Lab. izvještaj 7.

1. SSID: "30 Munroe St", SSID: "linksys12"
2. Za “30 Munroe St” je [Duration: 1464µs], a za “linksys12” [Duration: 456µs]
3. Izvorišna MAC adresa je (00:16:b6:f7:1d:51),
4. Odredišna je Broadcast (ff:ff:ff:ff:ff:ff)
5. BSS Id: CiscoLinksys\_f7:1d:51 (00:16:b6:f7:1d:51)
6. Tag: Extended Supported Rates 6(B), 9, 12(B), 18, 24(B), 36, 48, 54, [Mbit/sec]
7. Receiver address: CiscoLinksys\_f7:1d:51 (00:16:b6:f7:1d:51), Transmitter address: Intel\_d1:b6:4f (00:13:02:d1:b6:4f), Destination address: CiscoLinksys\_f4:eb:a8 (00:16:b6:f4:eb:a8). Izvorišna adresa je 192.168.1.109, a odredišna je 128.119.245.12. Adresa je vezana uz uređaj za prvi skok.
8. Receiver address: 91:2a:b0:49:b6:4f (91:2a:b0:49:b6:4f), Transmitter address: CiscoLinksys\_f7:1d:51 (00:16:b6:f7:1d:51), Destination address: 91:2a:b0:49:b6:4f (91:2a:b0:49:b6:4f). Adrese nisu iste.
9. Šalje se beacon frame i authentication frame
10. Poslano je 26 authentication frameova
11. Želi otvoren pristup
12. Da.
13. U t49, t53, t57, t62
14. Kartica podržava 24 Mb/s, a pristupna točka 54 Mb/s
15. U wireless1.pcap nisam pronašao CTS okvir.